ENTITY mux21 is

PORT(

I0, I1 : in bit\_vector(3 downto 0);

s : in bit;

Z : out bit\_vector(3 downto 0)

);

END mux21;

ARCHITECTURE concorrente of mux21 is

BEGIN

Z <= I0 WHEN S = '0' ELSE

I1;

END;